

**FACULTY OF INFORMATION AND COMMUNICATION TECHNOLOGIES**

**FALL 2023**

**CA EXAMINATION**

NAME: NDE HURICH DILAN


MATRICULE:ICTU20223351

EMAIL: nde.dilan@ictuniversity.edu.cm


TEL:+237694525931

**CCNA CA**


1-configure router1 with the hostname R1

****

2-configure router 2 with the hostname R2




3-Configure switch with the hostname SW1




The same command again for the last one


4-Configure the ip address of R1 according to the topology on the figure



5-Configure the ip address of R2 according to the topology on the figure




6-Give SW1 the management IP address 10.10.10.10/24:



7-The switch should have connectivity to other IP subnets via R2:




8-Verify that the switch can ping its default gateway:



It failed the first time so I tried again


9-Configure suitable descriptions for the connected devices

Let’s see configure one by one


Let’s see those descriptions


10-Verify that the link to R1 is on a full duplex mode and that the speed is set to 100Mbs



From here we can see the duplex and speed settings for f0/1 which is linked to R1

11-Manually configure full duplex and FastEthernet speed on the link to R2:

After everything is don ewe can check the results






12-Which version of IOS is you Cisco device using?

It seems like it’s version 12.2



13-Verify the directly attached Cisco neighbors using Cisco Discovery Protocol (CDP):




14-Prevent R1 from accessing information on SW1 via CDP

Let’s disable Cisco discovery protocol on the link between R2 and SW1




15-Flush the CDP cache on R1:




As shown below SW1 is no longer there.


16-Verify that R1 cannot see SW1 via CDP:




17-Let’s verify the status of the switch port connected to R2 with the **show ip interface brief** command.




18-Shut down the interface connected to R2 and issue a show ip interface brief command again.




19) Bring the interface up again:



20) and 21) Set the duplex to half on Switch 1 and Verify the state of the interface:



22-23) Set the duplex back to full duplex and Set the speed to 10 Mbps:



24)Check if the interface is still operational:



25)Check if the interface is operational on R2



The status is up/up

**SLIDE 14 QUESTION 1-5**

1-You have been given the 172.30.0.0/16 network. Your company requires 100 subnets with at least 500 hosts per subnet. What prefix length should you use?

To find the prefix length we should use, let’s find the number of borrowed bits.

We know that where x is the number of borrowed bits. So we have

And since we borrow 7bits, we will have a prefix length of 16+7=23.

2-What subnet does host 172.21.111.201/20 belong to?

To find the subnet it belongs to, we just need to find the network address of that subnet and to do that we can convert everything to binary and we will have :

1 0 1 0 1 1 0 0 . 0 0 0 1 0 1 0 1 . 0 1 1 0 1 1 1 1 . 1 1 0 0 1 0 0 1 since it’s a /20 it means that we have borrowed 4 bits so the last 12 bits are for the host, let’s make them all 0

1 0 1 0 1 1 0 0 . 0 0 0 1 0 1 0 1 . 0 1 1 0 0 0 0 0 . 0 0 0 0 0 0 0 0

Now if we convert it back we will have 172 . 21 . 96 . 0 Which is what we are looking for. **So the subnet mask is 172 . 21 . 96 .0**

3-What is the broadcast address of the network 192.168.91.78/26 belongs to?

It’s the same process as the last one but instead of turning all the host bits to **0** we will turn them into **1**.

So we have 1 1 0 0 0 0 0 0 . 1 0 1 0 1 0 0 0 . 0 1 0 1 1 0 1 1 . 0 1 0 0 1 1 1 0 and then

1 1 0 0 0 0 0 0 . 1 0 1 0 1 0 0 0 . 0 1 0 1 1 0 1 1 . 0 1 1 1 1 1 1 1 (note that the number of borrowed bits was 2)

**Converting it back to decimal give us 192.168.91.127/26**

4- You divide the 172.16.0.0/16 network into 4 subnets of equal size. Identify the network and broadcast addresses of the second subnet

To complete the task we need to find the network address of the first network and then deduce.

First we know that they are 4 subnets so 2 bits were borrowed, converting the address into binary give us : **1 0 1 0 1 1 0 0 . 0 0 0 1 0 0 0 0 . 0 0 0 0 0 0 0 0 0 . 0 0 0 0 0 0 0 0 (1st network address)**

to have the second network address we just add a 64 after 172.16 and in binary we get : **1 0 1 0 1 1 0 0 . 0 0 0 1 0 0 0 0 . 0 1 0 0 0 0 0 0 . 0 0 0 0 0 0 0 0 (2nd network address) In decimal it give us 172 . 16 . 64 . 0**

From there now we just turn the host part all to 1 to find the broadcast address, so in the end of the day the broadcast address is **1 0 1 0 1 1 0 0 . 0 0 0 1 0 0 0 0 . 0 1 1 1 1 1 1 1 . 1 1 1 1 1 1 1 1**

**which in decimal give 172 . 16 . 127 . 255.**

**So the** network and broadcast addresses of the second subnet are **172 . 16 . 64 . 0** and **172 . 16 . 127 . 255**

5- You divide the 172.30.0.0/16 network into subnets of 1000 hosts each. How many subnets are you able to make?

We know that we have 1000 hosts and the formula is

So .

**We have**

**And 64 subnets.**